**Metal Fabricated Channels, Struts, and Hardware Rebid**

**2025-06**

**Addendum #1**

**October 8, 2024**

Addendum #1 is to update Section 1.2.3, (f) of the IFB.

**Update:** Forming andholes drilled before steel is galvanized.

f) Steel support channels shall be according to ASTM A 653 (A 653M) (mild strip), and galvanized according to AASHTO M 232, Class B 2 after forming and drilling; aluminum support channel shall be “according to ASTM B 308 (B 308M), Alloy 6061-T6 or ASTM B 221 (B 221M), Alloy 6063-T6”.