Corrugated Metal Culverts

2020-09

# Addendum #1

Bid Due Date Extension/Pricing Table Revision

August 28, 2019

## Addendum #1 is to extend the bid due date and to revise the pricing table to correct line items 9 through 38.

* Bid due date extended to September 12, 2019 at 1:30 p.m. CST.

\*Reminder: Bids must be submitted to the address below: Illinois Department of Transportation

ATTN: Scott McKinnery

2300 S. Dirksen Parkway, Room 302

Springfield, IL 62764

* The pricing table has been revised. Line items 9 through 38 included a gauge specification that does not apply. The revisions have been made to the pricing pages attached to this notice. Please complete the revised pricing table and submit with your bid.
1. **PRICING**

### FORMAT OF PRICING:

* + 1. Vendor shall submit pricing in the format shown below, based on the terms and

conditions set forth in section 1 of this Contract.

* + 1. Pricing shall be submitted in the following format: A unit price and an extension

for each line item shall be quoted F.O.B. destination, freight prepaid to any Illinois

Department of Transportation location. Award will be made by line item to the

lowest cost and responsive and responsible bidder.

* + 1. Pricing shall be submitted in the following format:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Line No.** | **Description** | **Estimated Quantity** | **U/M** | **Unit Price** | **Extended Amount** |
| **1** | Perforated Corrugated Steel Sheet Metal Culvert, 18 Gauge, 6 Inch Diameter | 10 | Linear Foot | **$** | **$** |
| **2** | Plain Corrugated Steel Sheet Metal Culvert, 18 Gauge, 6 Inch Diameter | 10 | Linear Foot | **$** | **$** |
| **3** | Steel Connecting Band for 18 Gauge, 6 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 5 | Each | **$** | **$** |
| **4** | Plain Corrugated Steel Sheet Metal Culvert, 16 Gauge, 8 Inch Diameter | 5 | Linear Foot | **$** | **$** |
| **5** | Steel Connecting Band for 16 Gauge, 8 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 1 | Each | **$** | **$** |
| **6** | Steel Culvert End Section, Flared, 16 Gauge, for 8 Inch Diameter Pipe | 2 | Each | **$** | **$** |
| **7** | Plain Corrugated Steel Sheet Metal Culvert, 16 Gauge, 10 Inch Diameter | 35 | Linear Foot | **$** | **$** |
| **8** | Steel Connecting Band for 16 Gauge, 10 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 5 | Each | **$** | **$** |
| **9** | Plain Corrugated Steel Sheet Metal Culvert, 12 Inch Diameter | 1,300 | Linear Foot | **$** | **$** |
| **10** | Steel Connecting Band for 12 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 45 | Each | **$** | **$** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **11** | Plain Corrugated Steel Sheet Metal Culvert, 15 Inch Diameter | 9,000 | Linear Foot | **$** | **$** |
| **12** | Steel Connecting Band for 15 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 215 | Each | **$** | **$** |
| **13** | Steel Culvert End Section, Flared, for 15 Inch Diameter Pipe | 200 | Each | **$** | **$** |
| **14** | Plain Corrugated Steel Sheet Metal Culvert, 18 Inch Diameter | 6,200 | Linear Foot | **$** | **$** |
| **15** | Steel Connecting Band for 18 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 175 | Each | **$** | **$** |
| **16** | Steel Culvert End Section, Flared for 18 Inch Diameter Pipe | 175 | Each | **$** | **$** |
| **17** | Plain Corrugated Steel Sheet Metal Culvert, 21 Inch Diameter | 1,200 | Linear Foot | **$** | **$** |
| **18** | Steel Connecting Band for 21 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 22 | Each | **$** | **$** |
| **19** | Plain Corrugated Steel Sheet Metal Culvert, 24 Inch Diameter | 3,700 | Linear Foot | **$** | **$** |
| **20** | Steel Connecting Band for 24 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 280 | Each | **$** | **$** |
| **21** | Steel Culvert End Section, Flared, for 24 Inch Diameter Pipe | 235 | Each | **$** | **$** |
| **22** | Plain Corrugated Steel Sheet Metal Culvert, 30 Inch Diameter | 1,700 | Linear Foot | **$** | **$** |
| **23** | Steel Connecting Band for 30 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 60 | Each | **$** | **$** |
| **24** | Steel Culvert End Section, Flared, for 30 Inch Diameter Pipe | 75 | Each | **$** | **$** |
| **25** | Plain Corrugated Steel Sheet Metal Culvert, 36 Inch Diameter | 1,700 | Linear Foot | **$** | **$** |
| **26** | Steel Connecting Band for 36 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 60 | Each | **$** | **$** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **27** | Steel Culvert End Section, Flared, for 36 Inch Diameter Pipe | 65 | Each | **$** | **$** |
| **28** | Plain Corrugated Steel Sheet Metal Culvert, 42 Inch Diameter | 320 | Linear Foot | **$** | **$** |
| **29** | Plain Corrugated Steel Sheet Metal Culvert, 48 Inch Diameter | 500 | Linear Foot | **$** | **$** |
| **30** | Steel Connecting Band for 48 Inch Diameter Steel Pipe, 24 Inch Minimum Width | 25 | Each | **$** | **$** |
| **31** | Steel Culvert End Section, Flared, for 48 Inch Diameter Pipe | 30 | Each | **$** | **$** |
| **32** | Corrugated Steel Culvert Arch, 18 Inch Diameter, 22 Inch Span, 13 Inch Rise | 160 | Linear Foot | **$** | **$** |
| **33** | Corrugated Steel Culvert Arch, 21 Inch Diameter, 25 Inch Span, 16 Inch Rise | 330 | Linear Foot | **$** | **$** |
| **34** | Corrugated Steel Culvert Arch, 24 Inch Diameter, 29 Inch Span, 18 Inch Rise | 160 | Linear Foot | **$** | **$** |
| **35** | Corrugated Steel Culvert Arch, 30 Inch Diameter, 36 Inch Span, 22 Inch Rise | 470 | Linear Foot | **$** | **$** |
| **36** | Corrugated Steel Culvert Arch, 36 Inch Diameter, 43 Inch Span, 27 Inch Rise | 470 | Linear Foot | **$** | **$** |
| **37** | Corrugated Steel Culvert Arch, 48 Inch Diameter, 48 Inch Span, 36 Inch Rise | 470 | Linear Foot | **$** | **$** |
| **38** | Corrugated Steel Culvert Arch, 54 Inch Diameter, 65 Inch Span, 40 Inch Rise | 110 | Linear Foot | **$** | **$** |
| **39** | Arch Culvert Band, 18 Inch Diameter, 22 Inch Span, 13 Inch Rise | 5 | Each | **$** | **$** |
| **40** | Arch Culvert Band, 21 Inch Diameter, 25 Inch Span, 16 Inch Rise | 10 | Each | **$** | **$** |
| **41** | Arch Culvert Band, 24 Inch Diameter, 29 Inch Span, 18 Inch Rise | 5 | Each | **$** | **$** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **42** | Arch Culvert Band, 30 Inch Diameter, 36 Inch Span, 22 Inch Rise | 10 | Each | **$** | **$** |
| **43** | Arch Culvert Band, 36 Inch Diameter, 43 Inch Span, 27 Inch Rise | 10 | Each | **$** | **$** |
| **44** | Arch Culvert Band, 48 Inch Diameter, 48 Inch Span, 36 Inch Rise | 10 | Each | **$** | **$** |
| **45** | Arch Culvert Band, 54 Inch Diameter, 65 Inch Span, 40 Inch Rise | 5 | Each | **$** | **$** |
| **46** | Steel Culvert End Section, Flared, 16 Gauge for 12 inch Diameter Pipe | 8 | Each | **$** | **$** |
|  **47** |  Steel culvert end section, Flared, for 12 inch diameter pipe | 8 |  Each | **$** | **$** |
| **48** | Steel culvert end section, Flared, for 21 inch diameter pipe | 8 | Each | **$** | **$** |

 **GRAND TOTAL $\_\_\_\_\_\_\_\_\_\_\_\_\_**

* 1. **TYPE OF PRICING:** The Illinois Office of the Comptroller requires the State to indicate whether the contract value is firm or estimated at the time it is submitted for obligation. The total value of this contract is firm.
	2. **ESCALATION:** Contract prices must remain firm for the first twelve months of the contract. After this period and including potential renewal, the price(s) is subject to the following changes.

The Contractor may be allowed to adjust the purchase price of each line item in the event of changes in cost attributable to any of the following conditions: