Questions and Answers

Condition Rating Survey

CRSFY17

Addendum #4

1. **Section A.6.1. states the response deadline is December 29th. The is a very tight timeline considering that it runs through the holidays. Is it possible to obtain a timeline extension?** No
2. **Section B.4.3 states that “The Vendor must demonstrate their capability to provide a point cloud or similar data set for highway asset inventory” but does not go into specifics or accuracy requirements.**
	1. **Does IDOT require a LiDAR based point cloud?** The Department is not requiring a LiDAR based point cloud. If another independently proven type of dataset can meet the Department’s needs it will be considered.
3. **If so what density/specification/ accuracy**
	1. **Is a non-LiDAR calibrated 2D image acceptable as the “or similar”? Both methods can be used for length/height measurement and geo-referencing of assets and inventory.** Other means of highway asset inventory and measurement will be considered if it can be proven that a high degree of accuracy and precision with a low degree of error in measurement can be achieved. The vendor must demonstrate that a low variance in measurement between LiDAR and other means can be achieved. Accuracy for Structure and Overhead clearance is +- 1 inch.